A picture containing text, indoor, monitor, electronics

Description automatically generated

Yes, the application can show both RGB stream from the mono camera and depth map from the stereo camera simultaneously.

Max frame rate: 200

Resolution: 1920 × 2245